<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<packages>
<package name="1X03">
</package>
<package name="MOLEX-1X3">
</package>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="1X03_2MM">
</package>
<package name="1X03_1MM27">
</package>
</packages>
<symbols>
<symbol name="M03">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M03" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 3&lt;/b&gt;
Standard 3-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08232 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M03"/>
</gates>
<devices>
<device name="PTH" package="1X03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="1X03_1MM27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
