<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0.508" x2="28.428" y2="0.508" width="0" layer="20"/>
<wire x1="28.428" y1="0.508" x2="28.428" y2="33.198" width="0" layer="20"/>
<wire x1="28.428" y1="33.198" x2="2.54" y2="33.198" width="0" layer="20"/>
<wire x1="2.54" y1="33.198" x2="2.54" y2="0.508" width="0" layer="20"/>
<text>MSP430 NEBARNIX</text>
</plain>
<libraries>
<library name="TI_MSP430_v12">
<packages>
<package name="RHA40">
</package>
</packages>
</library>
<library name="XTAL">
<packages>
<package name="3MM2BY1MM5">
</package>
</packages>
</library>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="1X10">
</package>
<package name="1X08">
</package>
<package name="1X01">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="TI_MSP430_v12" package="RHA40" value="F22X4---RHA40"/>
<element name="U$1" library="XTAL" package="3MM2BY1MM5" value="ECX-31B"/>
<element name="JP2" library="SparkFun" package="1X10" value="M100.1"/>
<element name="JP4" library="SparkFun" package="1X08" value=""/>
<element name="JP3" library="SparkFun" package="1X08" value=""/>
<element name="JP1" library="SparkFun" package="1X08" value=""/>
<element name="JP5" library="SparkFun" package="1X01" value="M01PTH"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="20"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="30"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="N$7">
<contactref element="U$2" pad="31"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="39"/>
<contactref element="U$2" pad="38"/>
<contactref element="U$2" pad="14"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="19"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="U$2" pad="18"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$13">
<contactref element="U$2" pad="17"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="U$2" pad="16"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="N$15">
<contactref element="U$2" pad="15"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="N$16">
<contactref element="U$2" pad="12"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="11"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="U$2" pad="10"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="U$2" pad="9"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="U$2" pad="8"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="U$2" pad="7"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="U$2" pad="6"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="U$2" pad="5"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$23">
<contactref element="U$2" pad="40"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="U$2" pad="37"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="N$25">
<contactref element="U$2" pad="36"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$26">
<contactref element="U$2" pad="35"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$27">
<contactref element="U$2" pad="34"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="N$28">
<contactref element="U$2" pad="33"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$29">
<contactref element="U$2" pad="32"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$30">
<contactref element="U$2" pad="29"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="N$31">
<contactref element="U$2" pad="28"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="N$32">
<contactref element="U$2" pad="27"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="N$33">
<contactref element="U$2" pad="26"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$34">
<contactref element="U$2" pad="25"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="N$35">
<contactref element="U$2" pad="24"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="U$2" pad="23"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP3" pad="2"/>
<contactref element="U$2" pad="21"/>
</signal>
<signal name="N$37">
<contactref element="JP3" pad="1"/>
<contactref element="U$2" pad="22"/>
</signal>
<signal name="PE">
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$2" pad="13"/>
<contactref element="U$2" pad="TP"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
